| Home | Request Information | Warranty Information | Legal Information

Welcome: Guest Login Register View Cart Check Out Keep Shopping Account Information View Catalog Search Specials What's New |  |
Product Catalog / Geiger Mueller Tubes /
Name: TN1002-500V (5602-6W)
Code: GM Tubes
Description:
Radiation Detected | Alpha, Beta, Gamma, X-ray
Operating Voltage (volts) | 500
Operating Voltage Range (volts) | 475-675
Maximum Plateau Slope (%100 volts) | 10
Maximum Starting Voltage (volts) | 425
Maximum Dead Time (micro sec) | 100
Gamma Sensitivity Cs-137 (Cps/mGy/Hr) | 7500
Gamma Sensitivity Cs-137 (Cps/mR/Hr) | 65
Max. Background Shielded 50 mm Pb+3mm Al (CPM) | 30
Tube Capacitance (pf) | 3
Mica Window Density (mg/cm ^2) | 1.6-2.0
Effective Mica Window Diameter | 1.75/44.5
Overall Length (inch/mm) | 3.00/76.2
Overall Depth (inch/mm) | 0.61/15.5
Overall Diameter (inch/mm | 2.11/53.6 |  |
Filling Gasses | Ne, Ar, Halogens
Cathode Material | 400 Series SS
Recommended Min. Anode Resistor (meg Ohm) | 3.3
Gross Weight (grams) | 125
Operating Temperature Range, șC | -40 to 75
© Saint-Gobain Crystals & Detectors, 2001. All rights reserved |  |