| Home | Request Information | Warranty Information | Legal Information

Welcome: Guest Login Register View Cart Check Out Keep Shopping Account Information View Catalog Search Specials What's New |  |
Product Catalog / Geiger Mueller Tubes /
Name: T1504W (G1400)
Code: GM Tubes
Description:
Electrical Characteristics
Radiation Detected | Alpha, Beta, Gamma, X-ray
Maximum Starting Voltage (volts) | 325
Recommended Operating Voltage (volts) | 500
Operating Voltage Range (volts) | 450-650
Maximum Dead Time (micro-sec) | 90
Maximum Plateau Slope (% 100 volts) | 6
Maximum Anode Resistor (M) | 4.7
Recommended Anode Resistor (M) | 10
Gamma Sensitivity Cs137 (cps/mRhr) | 18
Max. Background Shielded 50mmPb+3mmAl (cpm) | 10
Tube Capacitance (pF) | 1.5
Weight (grams) | 6.0
Mechanical Characteristics
Active Length (inch/mm) | 1.53/ 39.0
Active Diameter (inch/mm) | 0.354/9.0
Cathode Material | 446 Stainless Steel
Cathode Wall Thickness (inch/mm) | 0.010/0.25
Areal Density (mg/cm2) | 250
Effective Window Diameter(inch/mm) | 0.354/9.0
Mica Window Thickness (inch/mm) | 1.5 - 2.0
Fill Gas | Ne/Ar+Halogen
Operating Temperature Range (șC) | -40 to +75
Type of Connector | PIN
© Saint-Gobain Crystals & Detectors, 2001. All rights reserved |  |